

**Keencut Excalibur 6000**

**Feature and benefits table**

|  |  |
| --- | --- |
| **Feature** | **Benefit** |
| Four blades cut along the same line | No need to alter production stops for different materials; it’s quick to set up for one-off jobs or repeatable volume cutting. |
| One-piece horizontal squaring arm | Ensures stability and accuracy. |
| Permanently mounted cutting tools | Lets you switch between cutting mount board, hardboard, glass, or acrylic in seconds. |
| Unique pressure-sensitive clamp | Protects delicate surfaces from damage. |
| PVC-covered arms | Create a stabilising non-scratch surface to safeguard expensive materials such as coated specialist glass.  |
| Easy Measuring Scale 65 degrees from the vertical | Provides easy visibility when setting the flip-in/out measuring stops.  |
| Lower Multi Tool head with unique ratchet system | Provides incremental cutting of thicker materials. |
| Upper Twin Wheel cutter | Cuts 3mm (1/8″) MDF in a single pass producing a clean finished edge. |
| Durable steel bearings | Ensures durability, zero play with perfect blade control, and low friction for an easy cut. |
| Easy access squaring system | Simplifies the initial set-up and maintains the Excalibur 6000 at 90-degree accuracy.  |
| Telescopic legs | Adjusts machine to perfect working height for each individual. |
| Integral counterbalance | Allows the Twin Wheel head to be left in place when loading and unloading materials. |
| Automatically disengaging blades | Ensures safety, ease of use, and operational speed. |
| Wall mounted or optional free-standing kit | Fits the available space. |
| Five-year guarantee | Reassurance of a comprehensive Keencut guarantee. |